F-18 construction
2 or 3 mm depron
1.  Build as 2 piece airplane
	A.  Fuselage and wing (make sure the wing sets flat, there is a slight kick about 		     1" from the end of the fuselage.  the wing must not go up on the kick up.  If 	      need adjust the wing slot)
	
	B.  Aft section:  stab, rudders and simulated jet motors.

	C.  Refer to pictures

2.  Before glueing the main fuselage/wing and aft section together install 
	Rx/motors/battery

3.  Try to get the f-18 to have a nice level glide before power flight.

good luck